**Measuring and Drawing Bearings**

Measure the bearing of B from A.

(a) (b)

(c) (d)



(e) (f)

Draw the following bearings:

(a) A point B on a bearing of 135o from A

(b) A point B on a bearing of 080o from A

(c) A point B on a bearing of 162o from A

Draw the following bearings:

(a) A point B on a bearing of 300o from A

(b) A point B on a bearing of 205o from A

(c) A point B on a bearing of 330o from A

**Measuring and Drawing Bearings**

Measure the bearing of B from A.

(a) (b)

(c) (d)



(e) (f)

Draw the following bearings:

(a) A point B on a bearing of 135o from A

(b) A point B on a bearing of 080o from A

(c) A point B on a bearing of 162o from A

Draw the following bearings:

(a) A point B on a bearing of 300o from A

(b) A point B on a bearing of 205o from A

(c) A point B on a bearing of 330o from A